.. zephyr:board:: sparkfun_thing_plus_matter_mgm240p

Overview
********

The MGM240P Mighty Sparkfun Think Plus Matter contains
a Wireless System-On-Chip from the EFR32MG24 family built on an
ARM Cortex®-M33F processor with excellent low power capabilities.

Hardware
********

- Based on the Series 2 EFR32MG24 SoC
- CPU core: 32-bit ARM® Cortex®-M33 core at 39 MHz
- Flash memory: 1536 kB
- RAM: 256 kB
- Supports Multiple 802.15.4 Wireless Protocols (Zigbee and OpenThread)
- Bluetooth Low Energy 5.3
- Crystals for LFXO (32 kHz) and HFXO (39 MHz).

For more information about the EFR32MG24 SoC and BRD2601B board, refer to these
documents:

- `EFR32MG24 Website`_
- `EFR32MG24 Datasheet`_
- `EFR32xG24 Reference Manual`_
- `MGM240P Datasheet`_
- `MGM240P Schematics`_

Supported Features
==================

.. zephyr:board-supported-hw::

Connections and IOs
===================

In the following table, the column **Name** contains Pin names. For example, PA2
means Pin number 2 on PORTA, as used in the board's datasheets and manuals.

+-------+-------------+-------------------------------------+
| Name  | Function    | Usage                               |
+=======+=============+=====================================+
| PA8   | GPIO        | LED0                                |
+-------+-------------+-------------------------------------+
| PA5   | USART0_TX   | UART Console EFM_BC_TX US0_TX       |
+-------+-------------+-------------------------------------+
| PA6   | USART0_RX   | UART Console EFM_BC_RX US0_RX       |
+-------+-------------+-------------------------------------+

The default configuration can be found in
:zephyr_file:`boards/sparkfun/thing_plus_matter_mgm240p/sparkfun_thing_plus_matter_mgm240p_defconfig`

System Clock
============

The EFR32MG24 SoC is configured to use the 39 MHz external oscillator on the
board.

Serial Port
===========

The EFR32MG24 SoC has one USART and two EUSARTs.
USART0 is connected to the board controller and is used for the console.

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

.. note::
   Before using the kit the first time, you should update the J-Link firmware
   in Simplicity Studio.

Flashing
========

The sample application :zephyr:code-sample:`hello_world` is used for this example.
Build the Zephyr kernel and application:

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: sparkfun_thing_plus_mgm240p
   :goals: build

Connect the sparkfun_thing_plus_mgm240p to your host computer using the USB port and you
should see a USB connection.

Open a serial terminal (minicom, putty, etc.) with the following settings:

- Speed: 115200
- Data: 8 bits
- Parity: None
- Stop bits: 1

Reset the board and you'll see the following message on the corresponding serial port
terminal session:

.. code-block:: console

   Hello World! _sparkfun_thing_plus_matter_mgm240p

Bluetooth
=========

To use the BLE function, run the command below to retrieve necessary binary
blobs from the SiLabs HAL repository.

.. code-block:: console

   west blobs fetch silabs

Then build the Zephyr kernel and a Bluetooth sample with the following
command. The :zephyr:code-sample:`bluetooth_observer` sample application is used in
this example.

.. zephyr-app-commands::
   :zephyr-app: samples/bluetooth/observer
   :board: sparkfun_thing_plus_matter_mgm240p
   :goals: build

.. _EFR32MG24 Website:
   https://www.silabs.com/wireless/zigbee/efr32mg24-series-2-socs#

.. _EFR32MG24 Datasheet:
   https://www.silabs.com/documents/public/data-sheets/efr32mg24-datasheet.pdf

.. _EFR32xG24 Reference Manual:
   https://www.silabs.com/documents/public/reference-manuals/efr32xg24-rm.pdf

.. _MGM240P Datasheet:
   https://cdn.sparkfun.com/assets/1/4/5/e/5/MGM240P-Datasheet.pdf

.. _MGM240P Schematics:
   https://cdn.sparkfun.com/assets/0/f/8/4/9/Thing_Plus_MGM240P.pdf
