; MEC174x SPI Image Generator configuration file
[SPI]
SPISizeMegabits = 128

[DEVICE]
TagAddr0 = 0
TagAddr1 = 0
; BoardID is used by a Boot-ROM feature named PlatformID. By default PlatformID
; is disabled. If PlatformID is enabled in OTP Boot-ROM will check the image
; BoardID value with an OTP PlatformID value. Load is aborted if the ID's do
; not match.
BoardID = 0x316

[IMAGE "0"]
ImageLocation = 0x2000
SpiFreqMHz = 24
SpiReadCommand = slow
SpiDriveStrength = 4
SpiSlewFast = false
SpiSignalControl = 0x00
IMG1BinFile = zephyr.bin
ImageRevision = 0
FwOffset = 0
IMG1LoadAddress = 0xB0000
IMG1EntryAddress = 0
UseECDSA = false
AuthenticateKeySelt = 5
AutoKeyRevEn = true
KeyRevPermission = 0xff
AutoRollBackProtEn = false
RollbackProtPerm031000 = 0
RollbackProtPerm063032 = 0
RollbackProtPerm095063 = 0
RollbackProtPerm127096 = 0
ECDSAPrivKeyFile = ECC384r.pem
ECDSAPrivKeyPassword = MCHPECC384r
FwEncrypt = false
AesGenECPubKeyFile = ECC384r_crt.pem
TagBuildNumber= 0
Comp0ProgDrvStrenEN = false
Comp0WritCmdTotByts = 0
Comp0ReadCmdByte = 0
Comp0WritCmdByte = 0
Comp0DrvValue = 0
Comp0DrvMask = 0
Comp1ProgDrvStrenEN = false
Comp1WritCmdTotByts = 0
Comp1ReadCmdByte = 0
Comp1WritCmdByte = 0
Comp1DrvValue = 0
Comp1DrvMask = 0
